Plain Elastomeric Pad

AASHTO LRFD Bridge Design Specifications

FDOT Structures Design Guidelines

Standard Specifications for Road and Bridge Construction

AASHTO LRFD Bridge Design Specifications
3.4.1 | Load Factors and Combinations – Load Factors and Load Combinations
3.5.1 | Permanent Loads – Dead Loads
3.6.1 | Gravity Loads – Vehicular Live Load
3.12 | Force Effects Due to Superimposed Deformations: TU, TG, SH, CR, SE
14.4 | Movements and Loads
14.6 | Requirements for Bearings
14.7.6 | Special Design Provisions for Bearings – Elastomeric Pads and Steel-Reinforced Elastomeric Bearings-Method A
14.8 s | Load Plates and Anchorage for Bearing

FDOT Structures Design Guidelines
Chap. 2 | Loads and Load Factors
6.5 | Bridge Bearings
6.5.1 | Bridge Bearings – Design of Bearings
6.5.2 | Bridge Bearings – Maintainability Requirements - Bearings
6.5.3 | Bridge Bearings – Lateral Restraint of Superstructures
6.5.3b | Bridge Bearings – Elastomeric Bearings
7.3.7 | Analysis and Design – Other Special Considerations
Chap. 9 | Bridge Cost Estimating

Standard Specifications for Road and Bridge Construction
Section 932-2 | Pads for Structures.
For current specifications: http://www.dot.state.fl.us/specificationsoffice/