## PROSECUTION AND PROGRESS - EQUIPMENT.

(REV 8-6-19) (7-19)

ARTICLE 8-4 is expanded by the addition of the following new Subarticle:

 **8-4.10 Equipment:** Equip vehicles and mobile equipment used on the project with a minimum of one class 2 amber or white flashing light that meets the Society of Automotive Engineers recommended practice SAE J845 and SAE J1318. The Engineer may require a white flashing light meeting the above requirements when conditions reduce the effectiveness of amber light (i.e., at night under high intensity discharge lights such as sodium vapor).

 Ensure all equipment safety devices recommended by the manufacturer are installed and properly maintained.

 Park vehicles and equipment not in use or left on the right-of-way overnight as close as possible to the right-of-way line and always outside of the applicable clear zone. Conduct service and supply operations as close to the right-of-way line as possible. Do not park equipment in the median, regardless of the width of the median, unless movement from the work area is determined by the Engineer to be prohibitive.

SUBARTICLE 8-5 is expanded by the following:

 All persons employed by the Contractor or Subcontractors working within the Department’s right-of-way must have Tier 1 Illicit Discharge Detection and Elimination (IDDE) training. The computer based training is provided by video on the following web page: <https://www.fdot.gov/maintenance/npdes-stormwater.shtm>.

 Provide a list of persons trained prior to submittal of the first invoice. Provide an updated list of new Contractor/Subcontractor employees annually thereafter.