Structures Design Office - 1998 Metric Standards CHANGES MADE FOR 1998 VERSION
Index No. | Description
I-099 | Changed the Table of Variables to follow Index No. S-119
100 | Added bubbles for End Conditions 2 and 3 and add a note End of Beams treatment for grade exceed 2%.
101 | Added bubbles for End Conditions 2 and 3 and add a note End of Beams treatment for grade exceed 2%.
S-102 | Removed Table of Beam Variables
S-103 | Removed Table of Beam Variables. Revised Bar Z in "Detail At End of Beam" view.
S-104 | Removed Table of Beam Variables
S-105 | Removed Table of Beam Variables and changed No. Required of Bar M to See Table
S-106 | Removed Table of Beam Variables and changed No. Required of Bar M to See Table
110 | Added bubbles for End Conditions 2 & 3 and add a note End of Beams treatment for grade exceed 2%.
S-111 | Removed Table of Beam Variables and changed No. Required of Bar M to See Table
S-112 | Removed Table of Beam Variables and changed No. Required of Bar M to See Table. Revised Bar Z in "Detail At End of Beam" view.
S-113 | Removed Table of Beam Variables and changed No. Required of Bar M to See Table
S-114 | Removed Table of Beam Variables and changed No. Required of Bar M to See Table
S-119 | New Sheet for New Table of Beam Variables
123 | Changed ASTM designation to Metric
S-128 | Changed ASTM designation to Metric
S-129 | Changed ASTM designation to Metric
S-130 | Changed ASTM designation to Metric
I-140 thru S-160 | New sheets for Florida U-Beams (FUB) with 1.2, 1.4, 1.6 and 1.8 m deep (21 sheets)
S-200 | Added Table of Required Pads, modified one Bearing Pad Notes and changed Index 200 to S-200
300 | Changed Loading from MS18 to M18
301 | Changed Loading from MS18 to M18
310 | Changed Loading from MS18 to M18
311 | Changed Loading from MS18 to M18
400 | Removed 95 from Note No. 6
S-401 | Added turn up at high side
S-402 | Added turn up at high side
403 | Added turn up at the high side, changed Sections 2, 3, 5 and changed Details A, B, C and Close-up of traffic barrier
500 | Changed conduit to Sch. 80, changed size from 63 to 53 mm, added pull box and 35 mm conduit from pull box to pilaster
510 | Changed 240 volts to 480 volts
600 | Changed Specification Section No. from 455-5.7 to 455-7.7
610 | Changed the key way to the direction of construction and stirrups
611 | Added a note for the key way and stirrups
612 | Added a note for the key way
S-613 | Added filter fabric
700 | Changed Pay Item Note, number and size of horizontal bars in the Traffic Barrier
710 | Changed Pay Item Note and the spacing of horizontal railing
720 | Changed Pay Item Note
CHANGES MADE FOR 1997 VERSION TO 1998 VERSION
Index No. | Description
800 | Changed density to unit weight
S-825 | New Sheet for Control Drawing - General Notes
S-900 | Changed Pay Item Note, provided Estimated Quantities block and also changed Index 900 to S-900
1300 | Added variable K to Type 41
2001 | Changed Note 8, added Note 12 and referenced Roadway Index 11037
S-2004 | Added Estimated Quantities block
2011 | Changed Notes 1, 8, 14 and added Notes 15 & 16 and referenced Roadway Index 11037 sheet 1 of 4
2011 | Changed Index No. from 2012 to 2011 and added a note to clarify Details D and E on Sheet No. 2 of 4
2011 | Changed Index No. 2013 to 2011 Sheet No. 3 of 4
2011 | Moved details from Index 2013 to 2011 Sheet No. 4 of 4
S-2012 | Added Estimated Quantities block, note and changed Index No. S-2014 to S-2012
2021 | Changed Note No. 8
2023 | Added Min. to some dimensions at Section G-G, and Details ’I’ and ‘J’
2024 | Changed definition of ‘UF’ on Section K-K, added Min. to some dimensions at Elevation, Details ‘N’ and ‘O’
2025 | Changed the designation of ‘UG’ and ‘LA’
S-2026 | Added Estimated Quantities block
CHANGES MADE FOR 1998 METRIC STANDARDS RELEASE 2
2001 | Revised Notes 11 from pay items 2125-1, 2400-4, and 2415-1 to no payment for the foundation.
2011 | Revised Notes 11 from pay items 2455-88 and 2455-122 to no payment for the foundation.
2021 | Revised Notes 11 from pay items 2455-88 and 2455-122 to no payment for the foundation.