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	FDOT Traffic Engineering Research Laboratory (TERL) 
Portable Regulatory Sign Compliance Matrix
	By signing this form, the applicant declares that he/she has read and understands the provisions of Section 990 of the FDOT Standard Specifications for Road and Bridge Construction and all implemented modifications. The requirements listed on this matrix are derived from Section 990 and are the basis for determining a product’s compliance and its acceptability for use on Florida’s roads.


	
FDOT Matrix Derived from Specification 990 (FA 8-28-25) CM-102-05 Rev 11.0
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	Date:
	Click here to enter a date.	Applicant’s 
Name (print):
	

	Manufacturer:
	     
	
	     

	Item, Model No.:
	     
	Signature:
	     



	
	
	** Greyed out rows in table below are for TERL use only **
	
	
	

	ID No
	Section
	Requirement
	Item Comply? (Yes/No/NA)
	Comments
(Applicant must provide information as indicated)
	TERL Evaluation Method

	The following compliance matrix criteria are for all portable regulatory signs.

	1
	990-3.1
	Device meets the physical display and operational requirements of the Manual on Uniform Traffic Control Devices (MUTCD) for Streets and Highways.
	[bookmark: Dropdown1]
	Applicant may provide comments in this field.
	 Document Review, Physical Inspection and Functional Inspection

	The following compliance matrix criteria (referencing the MUTCD) are from the MUTCD and are for all portable regulatory signs with a flashing beacon.

	2
	MUTCD Section 4S.01.03
	Beacons flash at a rate of not less than 50 or more than 60 times per minute.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and 
Functional Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 1), PRS003 (Step 2)
	     
	     
	Init.:      

	3
	
	The illuminated period of each flash is a minimum of ½ and a maximum of 2/3 of the total cycle.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 2)
	     
	     
	Init.:      

	4
	MUTCD Section 4S.01.04
	A beacon is not included within the border of a sign.
	
	Applicant may provide comments in this field.
	Physical Inspection

	
	
	TERL Test Cases (Steps): PRS002 (Step 1)
	     
	     
	Init.:      

	5
	MUTCD Section 4S.01.05
	The diameter of the flashing beacon signal indications is 12 inches.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and 
Physical Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 3), PRS002 (Step 2)
	     
	     
	Init.:      

	The following compliance matrix criteria (referencing the MUTCD) are from the MUTCD and are for all portable regulatory signs with a warning beacon.

	6
	MUTCD Section 4S.03.02
	Warning beacon has one or more signal sections of a standard traffic signal face with a flashing yellow signal indication in each section. 
	
	Provide the applicable compliance matrix from Specification 650 along with all supporting documentation that demonstrates this product meets this requirement. Alternately, provide the Approved Product List (APL) number if the signal assembly is APL listed.
	Document Review and
Physical Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 4), PRS002 (Step 3)
	     
	     
	Init.:      

	The following compliance matrix criteria (referencing the MUTCD) are from the MUTCD and are for all portable regulatory signs with a speed limit sign beacon.

	7
	MUTCD Section 4S.04.02
	Speed limit sign beacon has one or more signal sections of a standard traffic signal face with a flashing yellow signal indication in each section.
	
	Provide the applicable compliance matrices from Specification 650 along with all supporting documentation that demonstrates this product meets this requirement. Alternately, provide the Approved Product List (APL) number if the signal assembly is APL listed.
	Document Review and
Physical Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 5), PRS002 (Step 4)
	     
	     
	Init.:      

	8
	
	If two or more signal indications are used, they are alternately flashed.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and 
Functional Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 6), PRS003 (Step 3)
	     
	     
	Init.:      

	The following compliance matrix criteria (referencing the MUTCD) are from the MUTCD and are for all portable regulatory signs.

	9
	MUTCD Section 6G.02.02
	The sizes for portable regulatory signs, specifically speed limit signs (R2-1) are those in Table 6G-1.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and
Physical Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 7), PRS002 (Step 5)
	     
	     
	Init.:      

	The following compliance matrix criteria are for all portable regulatory signs.

	10
	990-3.1

	All assembly hardware less than 5/8 inch in diameter is type 304 or 316 passivated stainless steel.  Stainless steel bolts, screws and studs meet ASTM F593 and nuts meet ASTM F594.
	
	Provide statement of conformance from hardware supplier that shows the product meets this requirement.
	Document Review

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 8)
	     
	     
	Init.:      

	11
	
	All assembly hardware greater than or equal to 5/8 inch in diameter is galvanized. Bolts, studs, and threaded rod meet ASTM A307 and structural bolts meet ASTM F3125 Grade A325.
	
	Provide statement of conformance from hardware supplier that shows the product meets this requirement.
	Document Review

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 9)
	     
	     
	Init.:      

	12
	
	Electronic assemblies meet the requirements of NEMA TS 4.
	
	Provide the following:
· A third party test report that demonstrates compliance with this requirement.
· A completed Testing Laboratory and Report Checklist. 
· A completed NEMA TS4 2.2.3-2.2.6, 3.1.1 & 5.4 Checklist.
	Document Review

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 10)
	     
	     
	Init.:      

	13
	
	The controller and associated on-board circuitry are not affected by mobile radio, or any other radio transmissions.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 11)
	     
	     
	Init.:      

	14
	
	An operator’s manual is furnished with each unit.
	
	Provide a statement of conformance in this field.
	Compliance Matrix Review

	
	
	TERL Test Cases (Steps): PRS001 (Step 12)
	     
	     
	Init.:      

	15
	
	All portable devices are permanently marked with the APL number, manufacturer’s name or trademark, model/part number, and date of manufacture or serial number.
	
	Applicant may provide comments in this field.
	Physical Inspection

	
	
	TERL Test Cases (Steps): PRS002 (Step 6)
	     
	     
	Init.:      

	16
	
	The trailer is delineated with retroreflective material, known as conspicuity material, in a continuous line on the face of the trailer as seen by oncoming road users.
	
	Applicant may provide comments in this field.
	Physical Inspection

	
	
	TERL Test Cases (Steps): PRS002 (Step 7)
	     
	     
	Init.:      

	17
	990-3.1.1.1
	The unit provides automatic recharging of power supply batteries to normal operating levels with meters showing charge.
	
	Applicant may provide comments in this field.
	Functional Inspection

	
	
	TERL Test Cases (Steps): PRS005 (Step 4)
	     
	     
	Init.:      

	18
	
	Solar array recovery time is accomplished in a maximum of three hours.
	
	Applicant may provide comments in this field.
	Functional Inspection

	
	
	TERL Test Cases (Steps): PRS005 (Step 4)
	     
	     
	Init.:      

	19
	990-3.1.1.2
	The photovoltaic unit is designed to provide 10 days of continuous operation without sunlight with a minimum of onsite maintenance.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and 
Functional Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 13), PRS004 (Step 4)
	     
	     
	Init.:      

	20
	 
	The battery is equipped with a battery controller to prevent overcharging and over-discharging; an external battery level indicator is provided.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and
Physical Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 14), PRS002 (Step 8)
	     
	     
	Init.:      

	21
	 
	The battery, controller, and power panel are protected from the elements and vandalism.
	
	Applicant may provide comments in this field.
	Physical Inspection

	
	
	TERL Test Cases (Steps): PRS002 (Step 9)
	     
	     
	Init.:      

	22
	 
	Automatic recharging of power supply batteries is provided with charge indicator meter.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and Physical Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 15), PRS002 (Step 10)
	     
	     
	Init.:      

	23
	 
	An AC/DC battery charger unit is provided.
	
	Applicant may provide comments in this field.
	Physical Inspection

	
	
	TERL Test Cases (Steps): PRS002 (Step 11)
	     
	     
	Init.:      

	24
	990-3.1.2
	The display housing assembly is weather tight.
	
	Provide a statement of conformance in this field.
	Compliance Matrix Review

	
	
	TERL Test Cases (Steps): PRS001 (Step 16)
	     
	     
	Init.:      

	25
	 
	The display assembly is equipped with an automatic dimming operational mode capable of a minimum of 50 percent dimming and a separate manual dimmer switch.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and 
Functional Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 17), PRS006 (Steps 2, 3, 5)
	     
	     
	Init.:      

	26
	 
	The display panel background and frame for the display assembly is painted flat black and meets Federal Specification TT-E-489.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 18)
	     
	     
	Init.:      

	27
	 
	The regulatory speed sign panel for regulatory signs, when raised in the upright position, has a minimum height of 7 feet from the bottom of the regulatory sign panel to the ground.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and
Physical Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 19), PRS002 (Step 12)
	     
	     
	Init.:      

	28
	 
	The unit has an accessible mechanism to easily raise and lower the display assembly; a locking device is also provided to ensure the display panel will remain in the raised or lowered position.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and
Functional Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 20), PRS007 (Step 2)
	     
	     
	Init.:      

	29
	990-3.1.3
	Controller and control panel are housed in a weather, dust, and vandal resistant lockable cabinet.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and 
Physical Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 21), PRS002 (Step 13)
	     
	     
	Init.:      

	30
	990-3.1.4
	The support chassis is self-contained and self-supporting without the use of additional equipment or tools.
	
	Applicant may provide comments in this field.
	Physical Inspection

	
	
	TERL Test Cases (Steps): PRS002 (Step 14)
	     
	     
	Init.:      

	31
	
	The sign, power supply unit and all support systems are mounted on a wheeled trailer.
	
	Applicant may provide comments in this field.
	Physical Inspection

	
	
	TERL Test Cases (Steps): PRS002 (Step 15)
	     
	     
	Init.:      

	32
	
	The trailer is equipped with class-A lights, using a plug adaptor.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and
Physical Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 22), PRS002 (Step 16)
	     
	     
	Init.:      

	33
	
	The trailer is equipped with adjustable outrigger leveling pads, one on each of the four frame corners.
	
	Applicant may provide comments in this field.


	Physical Inspection

	
	
	TERL Test Cases (Steps): PRS002 (Step 17)
	     
	     
	Init.:      

	34
	
	The trailer can be set up at the site with its own chassis and outriggers, without being hitched to a vehicle.
	
	Applicant may provide comments in this field.
	Functional Inspection

	
	
	TERL Test Cases (Steps): PRS007 (Step 9)
	     
	     
	Init.:      

	35
	
	The trailer is equipped with fenders over the tires. 
	
	Applicant may provide comments in this field.
	Physical Inspection

	
	
	TERL Test Cases (Steps): PRS002 (Step 18)
	     
	     
	Init.:      

	36
	
	The trailer meets all equipment specifications set forth in Chapter 316 of the Florida Statutes, and by such rule, regulation or code that may be adopted by the Department of Highway Safety and Motor Vehicles.
	
	Applicant may provide comments in this field.

	Functional Inspection

	The following compliance matrix criteria (referencing Florida Statutes (F.S.)) are from Chapter 316, F.S. and are for trailers.

	37
	F.S. Section 316.221(1)
	The trailer is equipped with at least two taillamps mounted on the rear, which, when lighted as required in 316.217, F.S., emit a red light plainly visible from a distance of 1,000 feet to the rear.
	
	Applicant may provide comments in this field.
	Functional Inspection

	
	
	TERL Test Cases (Steps): PRS007 (Step 7)
	     
	     
	Init.:      

	38
	F.S. Section 316.221(2)
	Either a taillamp or a separate lamp is placed as to illuminate with a white light the rear registration plate of the trailer and render it clearly legible from a distance of 50 feet from the rear.
	
	Applicant may provide comments in this field.
	Functional Inspection

	
	
	TERL Test Cases (Steps): PRS007 (Step 6)
	     
	     
	Init.:      

	39
	F.S. Section 316.222(1)
	The trailer is equipped with two or more stop lamps meeting the requirements of 316.234(1), F.S.
	
	Applicant may provide comments in this field.
	Functional Inspection

	
	
	TERL Test Cases (Steps): PRS007 (Step 4)
	     
	     
	Init.:      

	40
	F.S. Section 316.222(2)
	The trailer is equipped with electric turn signal lamps meeting the requirements of 316.234(2), F.S.
	
	Applicant may provide comments in this field.
	Functional Inspection

	
	
	TERL Test Cases (Steps): PRS007 (Step 5)
	     
	     
	Init.:      

	The following compliance matrix criteria are for all portable regulatory signs.

	41
	990-3.4.1
	The sign panel assembly consists of a “SPEED LIMIT XX” sign panel and a “WHEN FLASHING” sign panel.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and Physical Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 23), PRS002 (Step 19)
	     
	     
	Init.:      

	42
	
	The sign panel folds down and can be pinned in place for towing; travel height does not exceed 80 inches.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and Physical Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 24), PRS002 (Step 20)
	     
	     
	Init.:      

	43
	
	Sign panel and light housing are constructed to allow the unit to be operated in the displayed position at speeds of 30 mph and transported at speeds of 65 mph.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 25)
	     
	     
	Init.:      

	44
	
	Unit is provided with a mechanism to raise and lower the sign panel and a device to lock the sign panel in the raised and lowered position.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and Functional Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 26), PRS007 (Step 2)
	     
	     
	Init.:      

	45
	990-3.4.2
	A pair of hooded PAR 46 LED advance warning flashing lamps, visible day or night at a distance of one mile with a flash rate of not less than 50 or more than 60 times per minute, is provided on each side of the top of the sign panel.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review, Physical Inspection and Functional Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 27), PRS002 (Step 21), PRS003 (Step 2), PRS007 (Steps 10, 11)
	     
	     
	Init.:      

	46
	
	The lamp lens is at least 5 3/4 inches in diameter.
	
	Applicant may provide comments in this field.
	Physical Inspection

	
	
	TERL Test Cases (Steps): PRS002 (Step 22)
	     
	     
	Init.:      

	47
	
	For solar powered units, the bulbs provide a 350-candlepower intensity for day use and an automatic reduction or dimming capacity for night use; the dimmed night operation provides adequate indication without excessive glare.
	
	Provide product literature, specifications, user manual, or similar information that shows the product meets this requirement.
	Document Review and Functional Inspection

	
	
	
	
	Indicate location of requested information in submittal.
	

	
	
	TERL Test Cases (Steps): PRS001 (Step 28), PRS006 (Step 5)
	     
	     
	Init.:      
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