Ad 27121 FPID 451022-1 
Frequently Asked Questions
0. This project will likely be a CAP Level 3 rather than a CAP Level 1 that was noted in the technical scope. 
0. Is a full drainage inventory required? 
2. No. Drainage structures should be reviewed and any recommendations for video and/or repair will be submitted to FDOT prior to Phase II. Only two (2) structures at this time are known to need evaluations.
0.  What ITS work is involved? 
3. Only the review of existing devices and installation of new devices.
0. Will any drainage redesigning be using an open or closed system? 
4. Closed; however, no redesign is anticipated at this time. 
0. Of the two median opens at Denny's, which is proposed to be closed?
5.  Median at Rdwy 1304000 MP 8.135 to 8.194 will be bi-directionalized. The median opening at Dennys will need to be redesigned to prevent turning issues. 
0. Were PHBs removed from the LRE? Why?
6.  Yes, PHBs were removed from this scope as a larger, more encompassing, project is being considered for the corridor in the future. 
0. Are we keeping the midblock crossing?
7.  No, the midblock will be part of the future project.
0. Are we correcting cross-slope issues?
8.  This should be evaluated and will be determined during Design.
0. Are we correcting lane shifts?
9. This will be evaluated during Design but is not currently in the scope or LRE. 
0. Is the corridor an emergency evacuation route?
10.  Yes
0. What permits, if any, have been pull/approved for the old mall reconstruction? Since 2024:
11. Utility - ALONG SR 684/US-41 and 44TH AVE CONNECTOR. FOR THE MADISON BRADENTON APTS BY THE OLD DESOTO SQUARE MALL
11. Utility - Crossing Under SR-684/US-41 and 44TH AVE CONNECTOR
11. Utility - AT MP 8.462 LT.
11. Utility - York Dr and Cortez Rd
11. Utility - MP 6.994
11. Withdrawn Construction Agreement
11. Drainage and Access - MP 7.081 - 7.673
11. General Use - MP 8.365 - 8.527
0. Is the contractor for the new apartments going to provide the sidewalk? 
12. Construction plans and permits have been published by the County and appear to include sidewalk. 
0. Is there potential for the proposed guardrail to be in conflict with the transmission pole?
13. This will need to be evaluated via SUE during Design.
0. Some landscaping has been planted near the PHBs. Will they be able to be relocated within the corridor?
14. This will need to be evaluated on a plant-by-plant basis per the Highway Landscape Guide.
0. Why was the PHB at the old mall removed in September of 2025?
15. Unknown at this time. 
0. Is Geotech going to be completed in-house?
16. Yes
0. Is survey going to be completed in-house?
17. No. The consultant will need to complete survey.
0. Will the consultant be responsible for scoping/videoing the drainage structures?
18. Yes
0. Will all structures be handled in-house?
19. Yes, including minor structures. 
0. Are there duplicate ITS items from another project which let in May 2026? Will duplicate items be removed from the LRE/scope?
20. Assume so. This will be reviewed during Design.
0. Has a warrant study been completed for the signal at 5th Street by the Department, apartment developer, or other entity?
21. Not that we are aware of at this time.
0. What caused all the patching along this corridor?
22. Unknown at this time. 
0. Will there be any preliminary UWHCA documents to review?
23. Not at this time. 
0. What level of TTCP will be needed?
24. To be determined during Design.
0. When were the PHBs installed? 
25. 2020 under FPID 446954-1
0. Is an up-to-date survey available? 
26. No. Survey will need to be completed by the consultant. 
0. Are the Leading Pedestrian Intervals (LPIs) along the corridor in sync with the use of PHBs?
27. The RSA requested for this to be evaluated. At this time, we do not see that this has been implemented. 
0. Will the speed be reduced to 35 mph or 40 mph?
28. 35mph
0. Has the lane shift concept already been implemented?
29. Per Rob Swann, only the lighting and optical pavement markings have been implemented. The shift of the striping to push the lanes west away from the transmission pole has not changed yet. 
0. Has the mid-block crossing gone to traffic ops and safety to be vetted? Why was the midblock crossing deleted from the LRE?
30. There will be no midblock on this project; the midblock will be added to the larger future project
0. Will the consultant provide traffic counts, will the Department, or has it already been completed?
31. A traffic count was conducted in 2019; unless Traffic Ops has been working on an additional study which has not been provided.
0. Is there a timing report or other timing coordination information that can be provided?
32. No. This will need to be evaluated during Design.
0. Will Constructability information be provided?
33. This will be discussed during the MOT and Constructability meeting during the Design phase of the project.
0. Exceptions were observed on the signed and sealed typical section package. Are these areas excepted from this project? What was the purpose of the exceptions?
34. It was clarified by our 4P group that these were intended to be labeled as equations rather than exceptions to denote changes in roadway identification. The TSP is being updated and resigned.
0. Has a Title Search for Right of Way been conducted at the North side of the 5th Street signal as it appears there's an easement there? Are we able to ensure correct reconstruction of the project?
35. Title Search will only be conducted if ROW is deemed necessary. There is no ROW phase on this project. 
0. Is it possible to extend the turn lanes to create the correct deceleration lengths?
36. This is a concept that can be discussed during Design.
0. Will Minor Project Type 4.1.1 be removed?
37. Yes, all structures are being handled in-house. 
0. Will 44th Ave after the beginning of the curve at Old Desoto Mall be included in this project?
38. Yes, please review project limits. 
0. Are we able to mill and resurface select lanes and areas rather than the entire thing? For example, where the PHBs were put in, the pavement is new; can these areas be exempt?
39. This can be discussed during the DRIVE D/C and Design processes.
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