## RAISED PAVEMENT MARKERS AND BITUMINOUS ADHESIVE.

(REV 3-30-20) (7-20)

ARTICLE 706-1 is deleted and the following substituted:

706-1 Description.

Remove and properly dispose of existing Raised Pavement Markers (RPMs) and replace with new RPMs and adhesive as specified in the work document, producing a positive guidance system to supplement other reflective pavement markings.

ARTICLE 706-4 is expanded by the following:

All markers for each work document will be in place before starting the initial 45 day replacement period under traffic.

ARTICLES 706-6 and 706-7 are deleted and the following substituted:

706-6 Method of Measurement.

The quantities to be paid for will be the number of RPMs, removed, furnished and installed, completed and accepted.

706-7 Basis of Payment.

Payment will be made under the items specified in the Bid Price Proposal.